*PADS-LOGIC-V9.0-CP936* À´×Ô PADS LOGIC V9.5 µÄÉè¼Æµ¼³öÎÄ¼þ
*SCH*        GENERAL PARAMETERS OF THE SCHEMATIC DESIGN"

CUR SHEET    0              Current Active Sheet
USERGRID     100    10      Design and Label/Text grid settings
LINEWIDTH    10             Width items will be created with
CONNWIDTH    10             Width used to plot connections
BUSWIDTH     25             Width used to plot buses
BUSANGLE     25             Angle used when plotting buses
NNVISPWRGND  4              Pwr/Gnd netname visibility default flag
PCBFLAGS     10283          PCB Netlist and ECO options
PINNAMESIZE  97     10      Height and LineWidth used by pin names
TEXTSIZE     100    10      Height and LineWidth text will be created width
JOBTIME      0              Amount of time spent on this LOGIC design
DOTGRID      1000           Space in thous/inch between graphic dots
BACKUPTIME   5              Number of minutes between database backups
TIEDOTSIZE   25             Diameter of tiedot point
REFNAMESIZE  100    10      Height and LineWidth used by part ref. names
PARTNAMESIZE 100    10      Height and LineWidth used by part type names
PINNOSIZE    97     10      Height and LineWidth used by pin numbers
NETNAMESIZE  100    10      Height and LineWidth used by net names
REAL WIDTH   20             Widths greater then this are displayed real size
SHEET SIZE   B             
UNITS        0              Rules units type
JOBNAME      Air780EP_LUATOS.sch
NTXCOL 11 9
HIRCOL 14
LINCOL 14
TXTCOL 11 9
CONCOL 13
BUSCOL 13
PTXCOL 11 9
COMCOL 11
NMCOL  11 9
PNMCOL 11 9
PINCOL 11 9
NETCOL 11 9
FBGCOL 15 0
OFFREFVIEW   0              Offsheet references visibility default flag
OFFREFNUM    0              Offsheet references per line
SHEETNUMSEP  []             Sheet Number separators
FONT MODE   System
DEFAULT FONT "Regular Verdana"
BORDER NAME SIZEB
FIELDCOL 10 2

*CAM* PLOTTER SETTINGS 

*MISC*      MISCELLANEOUS PARAMETERS
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

LAYER	MILS
{
LAYER	0
{
LAYER_THICKNESS	0
DIELECTRIC	3.300000
}
LAYER	1
{
LAYER_NAME	¶¥Ãæ
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
ASSOCIATED_SILK_SCREEN	Ë¿Ó¡¶¥²ã
ASSOCIATED_PASTE_MASK	Öúº¸²ã¶¥Ãæ
ASSOCIATED_SOLDER_MASK	×èº¸²ã¶¥²ã
ASSOCIATED_ASSEMBLY	×°ÅäÍ¼¶¥²ã
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	2
{
LAYER_NAME	µ×Ãæ
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Ë¿Ó¡µ×²ã
ASSOCIATED_PASTE_MASK	Öúº¸²ãµ×²ã
ASSOCIATED_SOLDER_MASK	×èº¸²ãµ×²ã
ASSOCIATED_ASSEMBLY	×°ÅäÍ¼µ×²ã
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	3
{
LAYER_NAME	Layer_3
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	4
{
LAYER_NAME	Layer_4
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	5
{
LAYER_NAME	Layer_5
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	6
{
LAYER_NAME	Layer_6
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	7
{
LAYER_NAME	Layer_7
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	8
{
LAYER_NAME	Layer_8
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	9
{
LAYER_NAME	Layer_9
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	10
{
LAYER_NAME	Layer_10
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	11
{
LAYER_NAME	Layer_11
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	12
{
LAYER_NAME	Layer_12
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	13
{
LAYER_NAME	Layer_13
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	14
{
LAYER_NAME	Layer_14
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	15
{
LAYER_NAME	Layer_15
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	16
{
LAYER_NAME	Layer_16
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	17
{
LAYER_NAME	Layer_17
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	18
{
LAYER_NAME	Layer_18
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	19
{
LAYER_NAME	Layer_19
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	20
{
LAYER_NAME	Layer_20
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	21
{
LAYER_NAME	×èº¸²ã¶¥²ã
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	22
{
LAYER_NAME	Öúº¸²ãµ×²ã
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	23
{
LAYER_NAME	Öúº¸²ã¶¥Ãæ
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	24
{
LAYER_NAME	×ê¿×Í¼
LAYER_TYPE	DRILL
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	25
{
LAYER_NAME	Layer_25
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	26
{
LAYER_NAME	Ë¿Ó¡¶¥²ã
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	27
{
LAYER_NAME	×°ÅäÍ¼¶¥²ã
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	28
{
LAYER_NAME	×èº¸²ãµ×²ã
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	29
{
LAYER_NAME	Ë¿Ó¡µ×²ã
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	30
{
LAYER_NAME	×°ÅäÍ¼µ×²ã
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
}
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

RULES_SECTION	MILS
{
NET_CLASS	DATA
DESIGN	RULES
{
RULE_SET	(1)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	6
VIA_TO_TRACK	6
VIA_TO_VIA	6
PAD_TO_TRACK	6
PAD_TO_VIA	6
PAD_TO_PAD	6
SMD_TO_TRACK	6
SMD_TO_VIA	6
SMD_TO_PAD	6
SMD_TO_SMD	6
COPPER_TO_TRACK	6
COPPER_TO_VIA	6
COPPER_TO_PAD	6
COPPER_TO_SMD	6
COPPER_TO_COPPER	6
TEXT_TO_TRACK	6
TEXT_TO_VIA	6
TEXT_TO_PAD	6
TEXT_TO_SMD	6
OUTLINE_TO_TRACK	6
OUTLINE_TO_VIA	6
OUTLINE_TO_PAD	6
OUTLINE_TO_SMD	6
OUTLINE_TO_COPPER	6
DRILL_TO_TRACK	6
DRILL_TO_VIA	6
DRILL_TO_PAD	6
DRILL_TO_SMD	6
DRILL_TO_COPPER	6
SAME_NET_SMD_TO_VIA	6
SAME_NET_SMD_TO_CRN	6
SAME_NET_VIA_TO_VIA	6
SAME_NET_PAD_TO_CRN	6
MIN_TRACK_WIDTH	6
REC_TRACK_WIDTH	6
MAX_TRACK_WIDTH	6
DRILL_TO_DRILL	6
BODY_TO_BODY	6
SAME_NET_TRACK_TO_CRN	6
}
}
RULE_SET	(2)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
ROUTE_RULE	:
{
LENGTH_MINIMIZATION_TYPE	1
TRACE_SHARE	Y
VIA_SHARE	Y
AUTO_ROUTE	Y
RIPUP	Y
SHOVE	Y
ROUTE_PRIORITY	3
MAX_NUMBER_OF_VIAS	-1
VALID_LAYER	1
VALID_LAYER	2
VALID_VIA_TYPE	*USE_CURRENT*
}
}
RULE_SET	(3)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
HIGH_SPEED_RULE	:
{
MIN_LENGTH	0
MAX_LENGTH	50000
STUB_LENGTH	0
PARALLEL_LENGTH	1000
PARALLEL_GAP	200
TANDEM_LENGTH	1000
TANDEM_GAP	200
MIN_DELAY	0.000000
MAX_DELAY	10.000000
MIN_CAPACITANCE	0.000000
MAX_CAPACITANCE	10.000000
MIN_IMPEDANCE	50.000000
MAX_IMPEDANCE	150.000000
SHIELD_NET	*
SHIELD_GAP	200
MATCH_LENGTH_TOLERANCE	200
}
}
}
}

*FIELDS*    USER FIELDS


*SHT*   1 $$$NONE -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        4.170          Scale of window expansion
WINDOWCENTER 4368   2483    Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT


*LINES*      LINES ITEMS


*CAEDECAL*  ITEMS

PIN              34000 34000 100 10 100 10 4 1 0 0 0 1
TIMESTAMP 2006.04.20.04.32.51
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             32000 32000 100 10 100 10 4 2 0 0 0 1
TIMESTAMP 2009.01.07.08.09.03
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PINSHORT         34000 34000 100 10 100 10 4 1 0 0 0 1
TIMESTAMP 2006.04.20.02.47.03
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

AIR780EP_LUATOS_A 32000 32000 97 10 97 10 4 1 0 48 0 0
TIMESTAMP 2024.10.31.10.45.04
"Default Font"
"Default Font"
20 110 0 4 97 10 "Default Font"
REF-DES
20 60 0 6 97 10 "Default Font"
PART-TYPE
20 -50 0 6 97 10 "Default Font"
*
20 -180 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
-1600 1800 
-1600 -1800
1600  -1800
1600  1800 
-1600 1800 
T-1800 1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 -200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 -400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 -600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 -800  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 -1000 0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1800 -1200 0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-800  -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-600  -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-400  -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T200   -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  -1200 0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  -1000 0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  -800  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  -600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  -400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  -200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1800  1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T200   2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-400  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-600  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-800  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1000 2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-1000 -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -2000 90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

AIR780EP_LUATOS_B 32000 32000 97 10 97 10 4 1 0 36 0 0
TIMESTAMP 2024.10.31.10.45.04
"Default Font"
"Default Font"
950 1320 0 0 97 10 "Default Font"
REF-DES
840 1510 0 2 97 10 "Default Font"
PART-TYPE
740 1090 0 2 97 10 "Default Font"
*
730 1230 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
2100  0    
2100  2600 
0     2600 
0     0    
T-200  2050  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1850  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1650  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1450  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1250  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1050  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  850   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  650   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  450   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  1100  0 1 140 20 0 1 220 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  1250  0 1 140 20 0 1 220 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  1450  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  1650  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  1850  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  2050  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  2800  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  2800  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  2800  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   2800  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   2800  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  2200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  300   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2300  2200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  2800  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   2800  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

AIR780EP_LUATOS_C 32000 32000 97 10 97 10 4 1 0 25 0 0
TIMESTAMP 2024.10.31.10.45.04
"Default Font"
"Default Font"
750 920 0 0 97 10 "Default Font"
REF-DES
660 870 0 2 97 10 "Default Font"
PART-TYPE
620 740 0 2 97 10 "Default Font"
*
620 630 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
1700  0    
1700  1800 
0     1800 
0     0    
T-200  1600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   -200  90 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  2000  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1900  1600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0


*PARTTYPE*   ITEMS

AIR780EP_LUATOS UND  3   0   0     0
TIMESTAMP 2024.10.31.10.45.02
GATE 1 48 0
AIR780EP_LUATOS_A
1 0 L GND
2 0 L NC
3 0 L NC
4 0 L NC
5 0 L NC
6 0 L NC
7 0 L PWRKEY
8 0 L NC
9 0 L ADC0
10 0 L GND
11 0 L USIM_DAT
12 0 L USIM_RST
13 0 L USIM_CLK
14 0 L USIM_VDD
15 0 L RESET_N
16 0 L GPIO27/AGPIO
17 0 L MAIN_RXD
18 0 L MAIN_TXD
19 0 L GPIO22/AGPIO/WAKEUP
20 0 L GPIO24/AGPIO
21 0 L GPIO36
22 0 L GPIO1
23 0 L GPIO2
24 0 L VDD_EXT
25 0 L GPIO26/AGPIO
26 0 L GPIO33
27 0 L GND
28 0 L AUX_RXD
29 0 L AUX_TXD
30 0 L GPIO29
31 0 L GPIO30
32 0 L GPIO31
33 0 L GPIO32
34 0 L GND
35 0 L LTE_ANT
36 0 L GND
37 0 L GND
38 0 L DBG_RXD
39 0 L DBG_TXD
40 0 L GND
41 0 L GND
42 0 L VBAT
43 0 L VBAT
44 0 L NC
98 0 L NC
97 0 L GPIO16
95 0 L GND
96 0 L ADC1
GATE 1 36 0
AIR780EP_LUATOS_B
45 0 L GND
46 0 L GND
47 0 L GND
48 0 L GND
49 0 L NC
50 0 L GPIO37
51 0 L GPIO38
52 0 L GPIO35
53 0 L GPIO34
54 0 L GPIO3
55 0 L GPIO6
56 0 L GPIO7
57 0 L GPIO15
58 0 L GPIO14
59 0 L USB_DP
60 0 L USB_DN
61 0 L VBUS
62 0 L USIM2_CLK
63 0 L USIM2_RST
64 0 L USIM2_DAT
65 0 L USIM2_VDD
66 0 L I2C_SDA
67 0 L I2S_SCL
68 0 L NC
69 0 L NC
70 0 L GND
71 0 L GND
72 0 L GND
99 0 L GPIO23/AGPIO
100 0 L IO_VOLT_SET
101 0 L WAKEUP0
102 0 L GPIO20/AGPIO/WAKEUP
103 0 L NC
104 0 L NC
105 0 L NC
106 0 L GPIO25/AGPIO
GATE 1 25 0
AIR780EP_LUATOS_C
73 0 L GND
74 0 L NC
75 0 L NC
76 0 L ADC3
77 0 L ADC2
78 0 L GPIO28/AGPIO
79 0 L USIM_DET
80 0 L GPIO4
81 0 L GPIO5
107 0 L GPIO21/AGPIO/WAKEUP
108 0 L NC
109 0 L NC
89 0 L GND
90 0 L GND
91 0 L GND
92 0 L GND
93 0 L GND
94 0 L GND
82 0 L USB_BOOT
83 0 L SPI_CS
84 0 L SPI_MISO
85 0 L SPI_MOSI
86 0 L SPI_CLK
87 0 L NC
88 0 L GND



*PART*       ITEMS



U1-A         AIR780EP_LUATOS  3700  5300    0 0 97 10 97 10 4 1 48 0 0 0
"Default Font"
"Default Font"
20 110 0 4 97 10 0 "Default Font"
REF-DES
20 60 0 6 97 10 0 "Default Font"
PART-TYPE
20 -50 0 6 97 10 0 "Default Font"
*
20 -180 0 6 97 10 0 "Default Font"
*
"PCB DECAL" AIR780E
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1
33 140 20 0 1
34 140 20 0 1
35 140 20 0 1
36 140 20 0 1
37 140 20 0 1
38 140 20 0 1
39 140 20 0 1
40 140 20 0 1
41 140 20 0 1
42 140 20 0 1
43 140 20 0 1
44 140 20 0 1
45 140 20 0 1
46 140 20 0 1
47 140 20 0 1

U1-B         AIR780EP_LUATOS  8600  4200    0 0 97 10 97 10 4 1 36 0 0 0
"Default Font"
"Default Font"
950 1320 0 0 97 10 0 "Default Font"
REF-DES
840 1510 0 2 97 10 0 "Default Font"
PART-TYPE
740 1090 0 2 97 10 0 "Default Font"
*
730 1230 0 2 97 10 0 "Default Font"
*
"PCB DECAL" AIR780E
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1
33 140 20 0 1
34 140 20 0 1
35 140 20 0 1

U1-C         AIR780EP_LUATOS  13900 4400    0 0 97 10 97 10 4 1 25 0 0 0
"Default Font"
"Default Font"
750 920 0 0 97 10 0 "Default Font"
REF-DES
660 870 0 2 97 10 0 "Default Font"
PART-TYPE
620 740 0 2 97 10 0 "Default Font"
*
620 630 0 2 97 10 0 "Default Font"
*
"PCB DECAL" AIR780E
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1


*BUSSES*


*OFFPAGE REFS*


*TIEDOTS*


*CONNECTION*


*NETNAMES*


*END*     OF ASCII OUTPUT FILE